Orangeburg Mud Bog

Rules & Classes

A Class – 0 – 36” DOT Tires

* 0 – 36” non cut DOT tires
* NO power adders (nitrous or forced induction)
* Roll cage and at least 4-point harness is required
* Helmet, neck brace and fire suit required
* Rear mounted kill switch and pull point are required
* Fire extinguisher required
* Minor trimming for tire clearance is allowed

B Class – 0 – 39.5” DOT Tires

* 0 – 39.5” non cut DOT tires
* NO power adders (nitrous or forced induction)
* Roll cage and at least 4-point harness is required
* Helmet, neck brace and fire suit required
* Rear mounted kill switch and pull point are required
* Fire extinguisher required
* Minor trimming for tire clearance is allowed

C Class – 0 – 44” DOT Tires

* 0 – 44” non cut DOT tires
* NO power adders (nitrous or forced induction)
* Roll cage and at least 4-point harness is required
* Helmet, neck brace and fire suit required
* Rear mounted kill switch and pull point are required
* Fire extinguisher required
* Minor trimming for tire clearance is allowed

1 Ton V-Tread

* 1-ton axles with any v-tread tractor tires
* Any power adder is allowed
* Helmet, neck brace and fire suit required
* Full roll cage and at least 4-point harness is required
* Rear mounted kill switch and pull point are required
* Fire extinguisher required

Mega Truck

* 2.5-ton axles with any v-tread tractor tires
* Any power adder is allowed
* Helmet, neck brace and fire suit required
* Full roll cage and at least 4-point harness is required
* Rear mounted kill switch and pull point are required
* Fire extinguisher required

Street Class

* Any street legal truck with non-cut DOT tires
* Stock body (no fiberglass body parts unless factory)
* NO Gutting allowed
* NO power adders (nitrous or forced induction)
* Helmet and neck brace required
* Full exhaust with muffler (no open headers)
* Rear mounted pull point required

Consistency

* Helmet and neck brace required
* Anything goes run what you got
* Driver with closest two times wins